1. ERCP table radiation protective screen must be made of material equivalent to 0.50 mm PB lead.


1. ERCP table radiation protective screen must be made of material equivalent to 0.50 mm PB lead.
3. Ercp table lead screen should provide 3-sided protection.
3. Ercp table lead screen should provide 3-sided protection.
Left side 200*60cm
Left side 200*60cm
The front side should consist of skirts measuring 60*70 cm.
4. Skirts should consist of a combination of 30-35 cm fringes. The eaves should overlap each other to prevent radiation leakage through them.
5. 6 pieces of 10 size velcro should be made on the table. And it should completely surround the table.
7. It must be made of rubber or vinyl material that will not break against the use of protective material.
7. It must be made of rubber or vinyl material that will not break against the use of protective material.
8. Product installation will be the responsibility of the manufacturer.
9. The table protective curtain must be wipeable.
There must be a module c2 and module b certificate that they have received from an independent auditor in accordance with the regulations.
There must be a module c2 and module b certificate that they have received from an independent auditor in accordance with the regulations.
11. The bidder must have a Medical Device Sales Center Authorization Certificate.
12. The manufacturer must have ISO 9001 AND ISO 13485 certificates.
13. The material must be guaranteed for 2 (two) years against manufacturing and workmanship defects.
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