




X RAY PROTECTIVE PREGNANT PROTECTIVE lead Apron TECHNICAL SPECIFICATION

1. LEAD APRON SHOULD PROVIDE PROTECTION AGAINST RADIATION EQUIVALENT TO Pb LEAD ON THE FRONT.

2. It should be strapped over the shoulders. It should be designed to protect the abdominal area.

3. For ergonomic use and long life of the lead apron, the inner fabric covering and fabric color of the apron and the outer fabric covering and color should be different.

4. The apron label must contain manufacturer information, vendor information, size information, production date, lot number and barcode number.

5. The protective lead material must be light, homogeneous, thin and multi-layered to ensure flexibility.

6. For pregnant protectors, it must be produced and certified in accordance with the Personal Protective Equipment Regulation (Official Gazette dated 01 May 2019 and numbered 30761, new regulation (EU) 2016/425

7. In accordance with the old standards for the products, article 11 a article 11 b certificate should not be submitted. These documents have become obsolete and documents must be submitted for the sale of products certified according to the new revision.

8. There must be full approval and test reports for the production of the product. It should offer this when requested.

9. There must be an internationally valid OHSAS 18001:2007 certificate for the production of radiation protective products from an accredited institution for the production of the product.

10. There must be an internationally valid OHSAS 18001:2007 certificate for the production of radiation protective products from an accredited institution for the production of the product.

11. There must be a separate test certificate or certificate of conformity for the product obtained from a department in Türkiye.
12. Manufacturers must have a domestic product certificate. It must be submitted in the file.

13. The fabric used must be waterproof, easy to wipe for long-term use and hygiene. The piping of the apron must be waterproof.

14. The fabric used must be waterproof, easy to wipe for long-term use and hygiene. The piping of the apron must be waterproof.

15. The manufacturer must provide a 2 (two) year warranty against production defects of lead aprons.

16. Color selection should be possible for lead aprons.





